Request for proposal

Fabrication and Installation of Metal Class C Grating

Guyana Shore Base Inc. hereby invites interested companies to submit proposals for the Fabrication and Installation of Metal Grating.

**Scope of Works**

**Fabrication**

* Fabrication of **Class C** Grating Panels in accordance with the Drawing **EDGD-A-105**.
* The quantity of grating panels is to be sufficient to cover the external Northern, Eastern and Western building boundaries as per Drawing **P7W-A-101.** Site survey is required.
* All materials, equipment and manpower for fabrication are to be supplied by the contractor.
* Gratings are to be fabricated from material that will ensure Class C load bearing capacity of gratings.
* Coated with red oxide primer to a minimum DFT of 80 µm.

**Installation**

* To be installed as per site layout shown in Drawing **P7W-A-101.**
* Transportation of fabricated gratings to site is to be done by the contractor.
* Contractor is to supply onsite labour, materials, and equipment to facilitate any on site modifications required during installation.
* Daily housekeeping and proper disposal of waste materials during installation and at the end of the project is a must.
* Adherence to GYSBI’s guidelines and policies during operation on site is a must.


**Certification**


* 40% random testing of grating panels to show that the fabricated gratings are in conformity with Class C grating loading specification.
* Certification of conformity is to be supplied.

**Instructions to Bidders**

1. Proposals are to be submitted along **Valid Business Registration or equivalent, Valid GRA & NIS Compliance, Local Content Certificate.**
2. Proposal and documents must be submitted to the e-mail address below **on or before March 1st, 2023.**

Email: **tenders@gysbi.com**

****

****