Request for proposal

Installation of Reinforced Concrete Trench Drain

Guyana Shore Base Inc. hereby invites interested companies to submit proposals for the INSTALLATION OF REINFORCED CONCRETE TRENCH DRAIN.

**Scope of Works**

* Site survey to ascertain BOQ and exact length of RC drain, see Drawing **P7W-A-101** for reference.
* Supply of requisite materials, equipment, and manpower to execute SOW.
* Excavation of Soil
* Compaction of subgrade.
* Supply and installation of vapour barrier.
* Supply and installation of supporting form work and shutters for casting of concrete drain.
* Supply and installation of 2” cement sand blinding.
* Supply and installation of requisite rebars as outlined per Drawing **P7WAD-A-107.**
* Supply of and pouring of **4000 Psi** concrete for RC drain.
  + Supply of Slump Testing.
  + Supply of Cube Testing.
    - Supply of Test results.
* Site survey and control to ensure correct drain elevation profile is maintained throughout construction.
* Backfilling and compaction of outer, external RC drain wall with crush run.
* Provision of dewatering as necessary.
* Upper profile of drain must be constructed to accommodate metal grating as outlined in Drawing **P7WAD-A-107.**
* Removal of form work and shutters.
* Adherence to GYSBI’s guidelines and policies.
* Daily housekeeping of worksite.
* Final site clearing and removal of all unwanted materials.


**Instructions to Bidders**

1. Proposals are to be submitted along **Valid Business Registration or equivalent, Valid GRA & NIS Compliance, Local Content Certificate.**
2. Proposal and documents must be submitted to the e-mail address below **on or before March 1st, 2023.**

Email: **tenders@gysbi.com**

**Diagram

Description automatically generated**

****